(footprint "TSOT-23-5_RIT" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "RT8059GJ5 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value TSOT-23-5_RIT (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -1.4478 -2.6416) (layer F.SilkS))
  (fp_text user "*" (at -0.6477 -1.5494) (layer F.Fab))
  (fp_text user "*" (at -0.6477 -1.5494 unlocked) (layer "F.Fab"))
  (fp_text user "*" (at -1.4478 -2.6416 unlocked) (layer "F.SilkS"))
  (pad "1" smd rect (at -1.1938 -0.9398) (size 1.3208 0.5588) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.1938 0) (size 1.3208 0.5588) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.1938 0.9398) (size 1.3208 0.5588) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 1.1938 0.9525) (size 1.3208 0.5588) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.1938 -0.9525) (size 1.3208 0.5588) (layers "F.Cu" "F.Paste" "F.Mask"))
)
