(module Package_SO:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 620A4557)
  (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "TSSOP SO")
  (attr smd)
  (fp_text reference REF** (at 0 -3.45) (layer F.SilkS))
  (fp_text value TSSOP-14_4.4x5mm_P0.65mm (at 0 3.45) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 14 smd rect (at 2.8625 -1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 2.8625 -1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 2.8625 -0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 2.8625 0) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 2.8625 0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 2.8625 1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.8625 1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.8625 1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.8625 1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.8625 0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.8625 0) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.8625 -0.65) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.8625 -1.3) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.8625 -1.95) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
