(footprint "TSSOP-16-1EP_4.4x5mm_P0.65mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "FE Package; 16-Lead Plastic TSSOP (4.4mm); Exposed Pad Variation BB; (see Linear Technology 1956f.pdf)")
	(tags "SSOP 0.65")
	(property "Reference" "REF**"
		(at 0 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSSOP-16-1EP_4.4x5mm_P0.65mm"
		(at 0 3.55 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.775 -2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -2.775 -1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -2.775 -0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -2.775 -0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -2.775 0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -2.775 0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -2.775 1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -2.775 2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at 2.775 2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at 2.775 1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at 2.775 0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at 2.775 0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at 2.775 -0.325)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at 2.775 -0.975)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at 2.775 -1.625)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 2.775 -2.275)
		(size 1.05 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at -0.735 -1.3425)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at -0.735 -0.4475)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at -0.735 0.4475)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at -0.735 1.3425)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.735 -1.3425)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.735 -0.4475)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.735 0.4475)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "17" smd rect
		(at 0.735 1.3425)
		(size 1.47 0.895)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)