(module Package_SO:TSSOP-8_4.4x3mm_P0.65mm (layer F.Cu) (tedit 61AD6981)
  (descr "TSSOP, 8 Pin (JEDEC MO-153 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "TSSOP SO")
  (attr smd)
  (fp_text reference REF** (at 0 -2.45) (layer F.SilkS))
  (fp_text value TSSOP-8_4.4x3mm_P0.65mm (at 0 2.45) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 8 smd rect (at 2.8625 -0.975) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.8625 -0.325) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.8625 0.325) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.8625 0.975) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.8625 0.975) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.8625 0.325) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.8625 -0.325) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.8625 -0.975) (size 1.475 0.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-8_4.4x3mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
