(module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 6469903A)
  (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
  (tags "Micro B USB SMD")
  (attr smd)
  (fp_text reference REF** (at 0 -3.3 180) (layer F.SilkS))
  (fp_text value USB_Micro-B_Molex_47346-0001 (at 0 4.6 180) (layer F.Fab))
  (fp_text user %R (at 0 1.2) (layer F.Fab))
  (fp_text user "PCB Edge" (at 0 2.67 180) (layer Dwgs.User))
  (pad 8 smd rect (at 1.55 1.2) (size 1 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.15 1.2) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 3.375 1.2) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -3.375 1.2) (size 1.65 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.4875 -1.375) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -2.4875 -1.375) (size 1.425 1.55) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
