(module VORA1010M4T (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOP-4_VIS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -6.3119 0) (layer Cmts.User))
  (fp_text user "0.022in/0.559mm" (at 6.3119 -1.27) (layer Cmts.User))
  (fp_text user "0.257in/6.528mm" (at 0 -4.8768) (layer Cmts.User))
  (fp_text user "0.054in/1.372mm" (at -3.2639 4.8768) (layer Cmts.User))
  (fp_text user "*" (at -3.5179 -2.9718) (layer F.SilkS))
  (fp_text user "*" (at -2.032 -2.3876) (layer F.Fab))
  (pad 1 smd rect (at -3.2639 -1.27) (size 1.3716 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.2639 1.27) (size 1.3716 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 3.2639 1.27) (size 1.3716 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.2639 -1.27) (size 1.3716 0.5588) (layers F.Cu F.Paste F.Mask))
)
