(footprint "VSON-8_3.3x3.3mm_P0.65mm_NexFET"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3.3x3.3x1 mm Body [VSON] http://www.ti.com/lit/ds/symlink/csd87334q3d.pdf")
	(tags "VSON 0.65")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "VSON-8_3.3x3.3mm_P0.65mm_NexFET"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.526 0.242 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.09 -0.61)
		(size 0.57 0.738)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.09 0.61)
		(size 0.57 0.738)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.86 -0.61)
		(size 0.57 0.738)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.86 0.61)
		(size 0.57 0.738)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 1.44 -0.9725)
		(size 0.63 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.44 -0.33)
		(size 0.63 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.44 0.33)
		(size 0.63 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.44 0.9725)
		(size 0.63 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.44 -0.97)
		(size 0.63 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.44 -0.33)
		(size 0.63 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.44 0.33)
		(size 0.63 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.44 0.97)
		(size 0.63 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.385 0)
		(size 1.9 2.45)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.371 -0.72) (xy 0.95 -0.72) (xy 0.95 -0.58) (xy 1.37 -0.58) (xy 1.37 -0.08) (xy 0.95 -0.08)
					(xy 0.95 0.08) (xy 1.37 0.08) (xy 1.37 0.58) (xy 0.95 0.58) (xy 0.95 0.72) (xy 1.37 0.72) (xy 1.37 1.225)
					(xy -0.95 1.225) (xy -0.95 -1.225) (xy 1.371 -1.225)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/VSON-8_3.3x3.3mm_P0.65mm_NexFET.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)