(footprint "Vishay_CNY70"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "package for Vishay CNY70 refective photo coupler/interrupter, https://www.vishay.com/docs/83751/cny70.pdf")
	(tags "Vishay CNY70 refective photo coupler")
	(property "Reference" "REF**"
		(at 1.4 -3.17 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_CNY70"
		(at 1.4 5.8 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "D"
		(at 2.8 1.27 0)
		(layer "Cmts.User")
	)
	(fp_text user "E"
		(at 0 1.27 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 1.5 1.27 0)
		(layer "F.Fab")
	)
	(fp_text user "Marking side"
		(at 4.33 1.27 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.156)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.8 2.54)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.8 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD8_3DMODEL_DIR}/OptoDevice.3dshapes/Vishay_CNY70.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)