(module Vishay_MOLD-3Pin (layer F.Cu) (tedit 5B888673)
  (descr "IR Receiver Vishay TSOP-xxxx, MOLD package, see https://www.vishay.com/docs/82669/tsop32s40f.pdf")
  (tags "IR Receiver Vishay TSOP-xxxx MOLD")
  (fp_text reference REF** (at 2.5 -2.25 180) (layer F.SilkS))
  (pad 1 thru_hole roundrect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.138))
  (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5.08 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/OptoDevice.3dshapes/Vishay_MOLD-3Pin.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
