(footprint WE-XHMA_8080 (layer F.Cu) (tedit 682BEB47)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at 0.0 -5.635 0) (layer F.SilkS))
  (fp_text value WE-XHMA_8080 (at 0.0 5.365 0) (layer F.Fab))
  (pad 1 smd rect (at 0.0 -2.5) (size 7.35 1.6) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 2 smd rect (at 0.0 2.5) (size 7.35 1.6) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.1)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.3 -1.65)
        (xy 4.3 -1.65)
        (xy 4.3 1.65)
        (xy -4.3 1.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.1)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.3 -1.65)
        (xy 4.3 -1.65)
        (xy 4.3 1.65)
        (xy -4.3 1.65)
      )
    )
  )
)