(module WEMOS_D1_mini_light (layer F.Cu) (tedit 5BBFB1CE)
  (descr "16-pin module, column spacing 22.86 mm (900 mils), https://wiki.wemos.cc/products:d1:d1_mini, https://c1.staticflickr.com/1/734/31400410271_f278b087db_z.jpg")
  (tags "ESP8266 WiFi microcontroller")
  (fp_text reference REF** (at 22 27) (layer F.SilkS))
  (fp_text value WEMOS_D1_mini_light (at 11.7 0) (layer F.Fab))
  (fp_text user %R (at 11.43 10) (layer F.Fab))
  (fp_text user "KEEP OUT" (at 11.43 -6.35) (layer Cmts.User))
  (fp_text user "No copper" (at 11.43 -3.81) (layer Cmts.User))
  (pad 2 thru_hole oval (at 0 2.54) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 5.08) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.62) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 10.16) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 12.7) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 0 15.24) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0 17.78) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 22.86 17.78) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 22.86 15.24) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 22.86 12.7) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 22.86 10.16) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 22.86 7.62) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 22.86 5.08) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 22.86 2.54) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (pad 16 thru_hole oval (at 22.86 0) (size 2 1.6) (drill 1) (layers *.Cu *.Mask))
  (model ${KICAD6_3DMODEL_DIR}/Module.3dshapes/WEMOS_D1_mini_light.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
    (offset (xyz 0 0 9.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 -180 0))
  )
  (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
    (offset (xyz 22.86 0 9.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 -180 0))
  )
  (model ${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
    (offset (xyz 22.86 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
