(footprint "WLCSP65_5.6x2.3x0.56mm" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "Grove - Vision AI Module V2.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (net_tie_pad_groups "A2" "B2")
  (fp_text reference "U1" (at 0 0.889 90) (layer "User.2"))
  (fp_text value "HX6538" (at 0 0 90) (layer "F.Fab"))
  (pad "A1" smd roundrect (at -0.8 -2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "A2" smd roundrect (at -0.4 -2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "A3" smd roundrect (at 0 -2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "A4" smd roundrect (at 0.4 -2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "A5" smd roundrect (at 0.8 -2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "B1" smd roundrect (at -0.8 -2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "B2" smd roundrect (at -0.4 -2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "B3" smd roundrect (at 0 -2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "B4" smd roundrect (at 0.4 -2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "B5" smd roundrect (at 0.8 -2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "C1" smd roundrect (at -0.8 -1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "C2" smd roundrect (at -0.4 -1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "C3" smd roundrect (at 0 -1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "C4" smd roundrect (at 0.4 -1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "C5" smd roundrect (at 0.8 -1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "D1" smd roundrect (at -0.8 -1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "D2" smd roundrect (at -0.4 -1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "D3" smd roundrect (at 0 -1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "D4" smd roundrect (at 0.4 -1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "D5" smd roundrect (at 0.8 -1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "E1" smd roundrect (at -0.8 -0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "E2" smd roundrect (at -0.4 -0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "E3" smd roundrect (at 0 -0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "E4" smd roundrect (at 0.4 -0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "E5" smd roundrect (at 0.8 -0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "F1" smd roundrect (at -0.8 -0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "F2" smd roundrect (at -0.4 -0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "F3" smd roundrect (at 0 -0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "F4" smd roundrect (at 0.4 -0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "F5" smd roundrect (at 0.8 -0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "G1" smd roundrect (at -0.8 0) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "G2" smd roundrect (at -0.4 0) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "G3" smd roundrect (at 0 0) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "G4" smd roundrect (at 0.4 0) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "G5" smd roundrect (at 0.8 0) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "H1" smd roundrect (at -0.8 0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "H2" smd roundrect (at -0.4 0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "H3" smd roundrect (at 0 0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "H4" smd roundrect (at 0.4 0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "H5" smd roundrect (at 0.8 0.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "J1" smd roundrect (at -0.8 0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "J2" smd roundrect (at -0.4 0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "J3" smd roundrect (at 0 0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "J4" smd roundrect (at 0.4 0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "J5" smd roundrect (at 0.8 0.8) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "K1" smd roundrect (at -0.8 1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "K2" smd roundrect (at -0.4 1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "K3" smd roundrect (at 0 1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "K4" smd roundrect (at 0.4 1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "K5" smd roundrect (at 0.8 1.2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "L1" smd roundrect (at -0.8 1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "L2" smd roundrect (at -0.4 1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "L3" smd roundrect (at 0 1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "L4" smd roundrect (at 0.4 1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "L5" smd roundrect (at 0.8 1.6) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "M1" smd roundrect (at -0.8 2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "M2" smd roundrect (at -0.4 2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "M3" smd roundrect (at 0 2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "M4" smd roundrect (at 0.4 2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "M5" smd roundrect (at 0.8 2) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "N1" smd roundrect (at -0.8 2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "N2" smd roundrect (at -0.4 2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "N3" smd roundrect (at 0 2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "N4" smd roundrect (at 0.4 2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (pad "N5" smd roundrect (at 0.8 2.4) (size 0.26 0.26) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.5)
    (thermal_bridge_angle 45))
  (model "${KICAD7_3DMODEL_DIR}/Package_BGA.3dshapes/BGA-90_8.0x13.0mm_Layout2x3x15_P0.8mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 0.2875 0.43 0.8))
    (rotate (xyz 0 0 0))
  )
)
