(module XAL1010-153MED (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_XAL1010_COC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0in/0mm" (at -6.3246 0) (layer Cmts.User))
  (fp_text user "0.315in/8.001mm" (at 6.3246 0) (layer Cmts.User))
  (fp_text user "0.258in/6.553mm" (at 0 -7.6708) (layer Cmts.User))
  (fp_text user "0.091in/2.311mm" (at -3.2766 7.0358) (layer Cmts.User))
  (pad 1 smd rect (at -3.2766 0) (size 2.3114 8.001) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.2766 0) (size 2.3114 8.001) (layers F.Cu F.Paste F.Mask))
)
