(footprint XCVR_H2U14W1H1A0400 (layer F.Cu) (tedit 68738AE2)
  (descr "")
  (attr smd)
  (fp_text reference REF** (at 7.375 -0.78 0) (layer F.SilkS))
  (fp_text value XCVR_H2U14W1H1A0400 (at 16.265 1.415 0) (layer F.Fab))
  (pad 1 smd rect (at -1.6 0.0) (size 0.6 1.6) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (pad 2 smd rect (at 1.6 0.0) (size 0.6 1.6) (layers F.Cu F.Mask F.Paste) (solder_mask_margin 0.102))
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.2 -1.0)
        (xy 3.3 -1.0)
        (xy 3.3 4.5)
        (xy -2.2 4.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.2 -1.0)
        (xy 3.3 -1.0)
        (xy 3.3 4.5)
        (xy -2.2 4.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 1.3 -0.8)
        (xy 1.3 0.8)
        (xy -1.3 0.8)
        (xy -1.3 -0.8)
      )
    )
  )
)