(module XGL5050-562MEC (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_XGL5050_COC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0in/0mm" (at -4.8514 0) (layer Cmts.User))
  (fp_text user "0.165in/4.191mm" (at 4.8514 0) (layer Cmts.User))
  (fp_text user "0.142in/3.607mm" (at 0 -5.1562) (layer Cmts.User))
  (fp_text user "0.041in/1.041mm" (at -1.8034 4.5212) (layer Cmts.User))
  (pad 1 smd rect (at -1.8034 0) (size 1.0414 4.191) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.8034 0) (size 1.0414 4.191) (layers F.Cu F.Paste F.Mask))
)
