(footprint "XIAO-nRF52840-SMD"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -9.445 -11.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "XIAO-nRF52840-SMD"
		(at 0.055 6.5 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at -8.945 10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at -8.945 10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -8.945 10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd roundrect
		(at -8.11 -7.62)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -8.11 -5.08)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -8.11 -2.54)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -8.11 0)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -8.11 2.54)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -8.11 5.08)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -8.11 7.62)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 8.055 7.62)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 8.055 5.08)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 8.055 2.54)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 8.055 0)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 8.055 -2.54)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 8.055 -5.08)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 8.055 -7.62)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd roundrect
		(at -4.5 -0.3135 180)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "16" smd roundrect
		(at -4.5 -2.2185 180)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "17" smd roundrect
		(at 3.755 9.2369 270)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "18" smd roundrect
		(at 5.66 9.2369 270)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 45)
	)
	(pad "19" smd circle
		(at -1.325 -8.5685)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd circle
		(at 1.215 -8.5685)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd circle
		(at -1.325 -6.0285)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd circle
		(at 1.215 -6.0285)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
)
