(footprint "XIAO-MG24-SMD"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 11.25 0.05 -90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "XIAO-MG24-SMD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd roundrect
		(at 7.62 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 5.08 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 2.54 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 0 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -2.54 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -5.08 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -7.62 -8.0825 90)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -7.62 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -5.08 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at -2.54 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "11" smd roundrect
		(at 0 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "12" smd roundrect
		(at 2.54 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "13" smd roundrect
		(at 5.08 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "14" smd roundrect
		(at 7.62 8.0825 270)
		(size 2.75 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "15" smd circle
		(at 3.81 5.000994 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd circle
		(at 1.27 5.000994 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd circle
		(at -1.27 5.000994 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd circle
		(at -3.81 5.000994 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd circle
		(at -3.81 -5.159006 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd circle
		(at -1.27 -5.159006 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd circle
		(at 1.27 -5.159006 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd circle
		(at 3.81 -5.159006 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd circle
		(at 8.65 -1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd circle
		(at 6.11 -1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd circle
		(at 3.57 -1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd circle
		(at 1.03 -1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "27" smd circle
		(at 1.03 1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "28" smd circle
		(at 3.57 1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "29" smd circle
		(at 6.11 1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "30" smd circle
		(at 8.65 1.27 90)
		(size 1.7 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "31" smd roundrect
		(at -4.974811 -1 180)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(pad "32" smd roundrect
		(at -4.974811 1 180)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-nRF52840 v15.step"
		(hide yes)
		(offset
			(xyz -1.778 -6.096 0.381)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeeduino XIAO SAMD21 v4.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO RP2040 v26.step"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO-ESP32-C3.step"
		(hide yes)
		(offset
			(xyz -1.7018 -6.096 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-ESP32S3 v2.step"
		(hide yes)
		(offset
			(xyz -1.778 -6.1722 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)