(footprint "Z4-D_CIP" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "Z4DGP406L-HF ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value Z4-D_CIP (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -3.5941 -2.5527) (size 4.0132 2.2606) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -3.5941 2.5527) (size 4.0132 2.2606) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 3.5941 2.5527) (size 4.0132 2.2606) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 3.5941 -2.5527) (size 4.0132 2.2606) (layers "F.Cu" "F.Paste" "F.Mask"))
)
