(footprint "JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal" (version 20240108) (generator "pcbnew") (generator_version "8.0")
  (layer "F.Cu")
  (descr "JST GH series connector, SM04B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST GH top entry")
  (property "Reference" "J7" (at 0 -3.9 180) (layer "F.SilkS")(hide yes))
  (property "Value" "Conn_01x04_Male" (at 0 3.9 180) (layer "F.Fab"))
  (property "Footprint" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Datasheet" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Description" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "LCSC" "C189895" (at 285 196 180) (layer "F.Fab")(hide yes))
  (attr smd)
  (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
  (pad "1" smd roundrect (at -1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at 0.625 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "4" smd roundrect (at 1.875 -1.85) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "MP" smd roundrect (at -3.725 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "MP" smd roundrect (at 3.725 1.35) (size 1 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
