(footprint "lambreta-MX1508" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "line_follower.kicad_sch")
  (property "Sheetname" "")
  (attr smd)
  (fp_text reference "H_Brg1" (at -0.1016 -11.049 90 unlocked) (layer "F.SilkS"))
  (fp_text value "lambreta-MX1508" (at 0 1 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole rect (at -10.0396 -18.4384) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "2" thru_hole oval (at -10.0396 -15.8984) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "3" thru_hole oval (at -7.0396 -10.8984) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "4" thru_hole oval (at -7.0396 -8.3584) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "5" thru_hole oval (at -7.0396 -5.8184) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "6" thru_hole oval (at -7.0396 -3.2784) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "7" thru_hole oval (at 7.3152 -10.8712) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "8" thru_hole oval (at 7.3152 -8.3312) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "9" thru_hole oval (at 7.3152 -5.7912) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
  (pad "10" thru_hole oval (at 7.3152 -3.2512) (size 1.7 1.7) (drill 1) (layers "*.Mask" "F.Cu" "In1.Cu" "B.Cu"))
)
