(module lm2907n (layer F.Cu)
  (fp_text reference REF** (at 3.81 7.62) (layer F.SilkS))
  (fp_text value N14A_TEX (at 3.81 7.62) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 10.668 0) (layer Cmts.User))
  (fp_text user "0.3in/7.62mm" (at 3.81 -4.3815) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 0 19.6215) (layer Cmts.User))
  (fp_text user "*" (at 0.762 0) (layer F.Fab))
  (fp_text user "*" (at 0 -1.524) (layer F.SilkS))
  (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 7.62 15.24) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 7.62 12.7) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 7.62 10.16) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 7.62 7.62) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 7.62 5.08) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
)
