(footprint "pam8403" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS"))
  (fp_text value "pam8403" (at 0 1 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole circle (at -7.62 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -5.08 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -2.54 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 5.08 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 7.62 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 7.62 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 5.08 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at -5.08 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at -7.62 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
