(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 4.69)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user "Nutzer.1")
		(51 "User.2" user "Nutzer.2")
		(52 "User.3" user "Nutzer.3")
		(53 "User.4" user "Nutzer.4")
		(54 "User.5" user "Nutzer.5")
		(55 "User.6" user "Nutzer.6")
		(56 "User.7" user "Nutzer.7")
		(57 "User.8" user "Nutzer.8")
		(58 "User.9" user "Nutzer.9")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x000d0fc_ffffffff)
			(plot_on_all_layers_selection 0x0001000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/home/crypt/Desktop/gedm-evoII-kicad/G-EDM-EVOII-Kicad-projects/gerber-files-evoII-v0.2/pulseboard-evoII/")
		)
	)
	(net 0 "")
	(net 1 "5v")
	(net 2 "+48V")
	(net 3 "spark-minus-to-drain")
	(net 4 "5v-optoout")
	(net 5 "Net-(D1-A)")
	(net 6 "Net-(D3-A)")
	(net 7 "Net-(D6-A)")
	(net 8 "Net-(D7-A)")
	(net 9 "Net-(D13-A)")
	(net 10 "12vpower")
	(net 11 "unconnected-(IC5-NC_1-Pad1)")
	(net 12 "Net-(IC5-CATHODE)")
	(net 13 "unconnected-(IC5-NC_2-Pad4)")
	(net 14 "Net-(D18-K)")
	(net 15 "GND2")
	(net 16 "unconnected-(IC5-VB-Pad7)")
	(net 17 "pwm-in")
	(net 18 "Net-(D1-K)")
	(net 19 "Net-(VR1-CCW)")
	(net 20 "Net-(J7-Pin_2)")
	(net 21 "to-sb-esp-gnd1")
	(net 22 "Net-(U3-SS)")
	(net 23 "Net-(U3-COMP)")
	(net 24 "Net-(C20-Pad1)")
	(net 25 "18V")
	(net 26 "Net-(U3-RT)")
	(net 27 "Net-(U3-FB)")
	(net 28 "Net-(U1-OUTH)")
	(net 29 "unconnected-(U1-EN-Pad1)")
	(net 30 "unconnected-(U3-NC-Pad15)")
	(footprint "Library:INF-PG-TO247-3"
		(layer "F.Cu")
		(at 62.86 73.1 -90)
		(descr "Original name INF-PG-TO247-3\n\nMax Component Height - 25.57mm")
		(property "Reference" "Q3"
			(at -3 -9.25 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "IMW65R050M2H "
			(at 0.25 2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:INF-PG-TO247-3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ooo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OptiMOS 3 Power-Transistor, VDS 100V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 -5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D7-A)")
			(pinfunction "GATE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "DRAIN")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 0 5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "SOURCE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 60.37755 59.953 180)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at -2.665 3.0988 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7Ohm RC2512JK-7W4R7L"
			(at 0 2.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 8 "Net-(D7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 18 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 92.5 113.6 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C14"
			(at -2.834 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "C100pf500v KERKO-500 100P"
			(at 2.5 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.8)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Altech:Altech_AK100_1x02_P5.00mm"
		(layer "F.Cu")
		(at 43.1 29.7 180)
		(descr "Altech AK100 serie terminal block (Script generated with StandardBox.py) (https://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK100 serie connector")
		(property "Reference" "J4"
			(at -0.35 -6.09 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 5.25 180)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Altech:Altech_AK100_1x02_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -0.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D18-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK100_1x02_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:SOP254P1016X460-8N"
		(layer "F.Cu")
		(at 97.028 32.2072 180)
		(descr "6N136S-")
		(tags "Integrated Circuit")
		(property "Reference" "IC5"
			(at -4.1402 -6.3754 180)
			(layer "F.SilkS")
		)
		(property "Value" "6N137S"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "custom:SOP254P1016X460-8N"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC-IN 1-CH Transistor With Base DC-OUT 8-Pin DIP SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "6N136S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/6n136s/lite-on-technology?region=nac"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "6N136S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "859-6N136S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Lite-On/6N136S?qs=PByDJ0nQNwodpj4vLYO2Qg%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4.1402 -6.3754 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.55 -3.81 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(IC5-NC_1-Pad1)")
			(pinfunction "NC_1")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -4.55 -1.27 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "pwm-in")
			(pinfunction "ANODE")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.55 1.27 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(IC5-CATHODE)")
			(pinfunction "CATHODE")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -4.55 3.81 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "unconnected-(IC5-NC_2-Pad4)")
			(pinfunction "NC_2")
			(pintype "no_connect")
		)
		(pad "5" smd rect
			(at 4.55 3.81 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(pad "6" smd rect
			(at 4.55 1.27 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "5v-optoout")
			(pinfunction "VO")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 4.55 -1.27 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "unconnected-(IC5-VB-Pad7)")
			(pinfunction "VB")
			(pintype "no_connect")
		)
		(pad "8" smd rect
			(at 4.55 -3.81 270)
			(size 1.45 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "5v")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "6N136S.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 108.5596 62.9412 90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k RK73B2ETTD104J"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 6 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 50.0278 100.0506 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 1.3818 2.8702 0)
			(layer "F.SilkS")
		)
		(property "Value" "1% 1.0Kohm ERJ-U12F1001U"
			(at 0 2.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 2 "+48V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 19 "Net-(VR1-CCW)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 29.6 117)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H2"
			(at 3.1914 3.777 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 29.6 32)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "TerminalBlock_Altech:Altech_AK100_1x02_P5.00mm"
		(layer "F.Cu")
		(at 29.464 47.498 -90)
		(descr "Altech AK100 serie terminal block (Script generated with StandardBox.py) (https://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK100 serie connector")
		(property "Reference" "J6"
			(at -0.35 -6.09 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1776138-2 and 796641-2"
			(at 2.5 5.25 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Altech:Altech_AK100_1x02_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "796643-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN2_796643-2_TEC")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -0.5 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12vpower")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK100_1x02_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:logo"
		(layer "F.Cu")
		(at 67.3 86.7)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Library:logo"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 40.59435 59.3152 180)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at -2.6396 3.048 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7Ohm RC2512JK-7W4R7L"
			(at 0 2.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 7 "Net-(D6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 18 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:INF-PG-TO247-3"
		(layer "F.Cu")
		(at 83.3 73.3 -90)
		(descr "Original name INF-PG-TO247-3\n\nMax Component Height - 25.57mm")
		(property "Reference" "Q1"
			(at -3 -9.25 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "IMW65R050M2H "
			(at 0.25 2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:INF-PG-TO247-3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ooo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OptiMOS 3 Power-Transistor, VDS 100V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 -5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D1-A)")
			(pinfunction "GATE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "DRAIN")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 0 5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "SOURCE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 88.8746 31.9118 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10kOhm  WRIS-RSKS 560112120004"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 1 "5v")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 4 "5v-optoout")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 109.8296 46.4058 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R42"
			(at 3.5052 1.2192 0)
			(layer "F.SilkS")
		)
		(property "Value" "560Ohm RK73B2ATTD561J"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 9 "Net-(D13-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 1 "5v")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 56.179999 51.87 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1.1k"
			(at 0 1.65 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 24 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 64 53.7 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.68 -90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "18V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 46.629999 45.47)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "12vpower")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:DEGSONDG135T101602P1300AH"
		(layer "F.Cu")
		(at 73.22 115.83)
		(descr "DEGSON DG135T-10.16-02P-13-00AH-2")
		(tags "Connector")
		(property "Reference" "J17"
			(at 5.08 -2.73 0)
			(layer "F.SilkS")
		)
		(property "Value" "Degson DG135T-10.16-02P-13-00AH"
			(at 5.08 -2.73 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "custom:DEGSONDG135T101602P1300AH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Degson DG135T-10.16-02P-13-00AH pricing and available inventory."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "29.5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Degson"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DEGSON DG135T-10.16-02P-13-00AH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 -2.73 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -10.16)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 10.16 -10.16)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "DEGSON_DG135T-10.16-02P-13-00AH.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 49.879999 51.87 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "9.78k"
			(at 0 1.65 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 26 "Net-(U3-RT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm"
		(layer "F.Cu")
		(at 39.5 43.7388 -90)
		(descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
		(property "Reference" "C15"
			(at 4.826 -4.8006 -90)
			(layer "F.SilkS")
		)
		(property "Value" "220uf35v RD1V227M0811M160"
			(at 1.75 5.25 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12vpower")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole circle
			(at 3.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.6)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 83.8 40.3 180)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
		(property "Reference" "C19"
			(at 5.517277 5.5118 0)
			(layer "F.SilkS")
		)
		(property "Value" "470uf35v RD1V477M10016100"
			(at 2.5 6.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.4773 -2.041651 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12vpower")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.6)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 31.2 91.8 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C11"
			(at -2.5908 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "C100pf500v KERKO-500 100P"
			(at 2.5 2.5 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.8)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 105.9 116.3 -90)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D21"
			(at 0 -4.1 -90)
			(layer "F.SilkS")
		)
		(property "Value" "ES5GC"
			(at 0 4.2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "+48V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.4 0)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 15 "GND2")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 60.536321 47.320001)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "42.2k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 27 "Net-(U3-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 25 "18V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "F.Cu")
		(at 40.98795 64.065)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D6"
			(at -5.7042 1.2192 0)
			(layer "F.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -5.7042 1.2192 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 18 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 7 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "graphics:warning-high-voltage-10mm"
		(layer "F.Cu")
		(at 96.765729 87.098124)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "graphics:warning-high-voltage-10mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 29.5 97 180)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D14"
			(at 0 -4.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "ES5GC"
			(at 0 4.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0 270)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "+48V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.4 0 270)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 15 "GND2")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "F.Cu")
		(at 60.95975 64.6266)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D7"
			(at -5.715 1.1938 0)
			(layer "F.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -5.715 1.1938 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 18 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 8 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:TO255P460X1020X2008-3P"
		(layer "F.Cu")
		(at 89.916 44.704)
		(descr "3-Pin TO-220")
		(tags "Integrated Circuit")
		(property "Reference" "U2"
			(at 9.3734 -2.43355 90)
			(layer "F.SilkS")
		)
		(property "Value" "L7805"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "custom:TO255P460X1020X2008-3P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 9.3734 -2.43355 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.98 1.98)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12vpower")
			(pinfunction "IN")
			(pintype "power_in")
			(zone_connect 1)
			(thermal_bridge_width 1.2)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole circle
			(at 2.55 0)
			(size 1.98 1.98)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
			(thermal_gap 0.3)
		)
		(pad "3" thru_hole circle
			(at 5.1 0)
			(size 1.98 1.98)
			(drill 1.32)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5v")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "L7805CV.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:DEGSONDG135T101602P1300AH"
		(layer "F.Cu")
		(at 49.913288 115.483766)
		(descr "DEGSON DG135T-10.16-02P-13-00AH-2")
		(tags "Connector")
		(property "Reference" "J19"
			(at 5.08 -2.73 0)
			(layer "F.SilkS")
		)
		(property "Value" "Degson DG135T-10.16-02P-13-00AH"
			(at 5.08 -2.73 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "custom:DEGSONDG135T101602P1300AH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Degson DG135T-10.16-02P-13-00AH pricing and available inventory."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "29.5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Degson"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DEGSON DG135T-10.16-02P-13-00AH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 -2.73 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -10.16)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 10.16 -10.16)
			(size 3.3 3.3)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "DEGSON_DG135T-10.16-02P-13-00AH.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 33.274 105.918 -90)
		(descr "JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J7"
			(at 6.2992 6.5024 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 1.25 10.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 3.45 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 15 "GND2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 270)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 51.979999 51.87 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.68 -90)
			(layer "F.SilkS")
		)
		(property "Value" "300pF"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U3-COMP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 68.4 37.3 -90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
		(property "Reference" "C21"
			(at 2.5 -6.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uf35v RD1V477M10016100"
			(at 2.5 6.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "18V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:LM5157"
		(layer "F.Cu")
		(at 53.179999 46.620001)
		(tags "LM51571QRTERQ1 ")
		(property "Reference" "U3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LM51571QRTERQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:LM5157"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "LM51571QRTERQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RTE0016K")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "Designator161"
			(at -1.727256 -3.02257 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.4 -0.750001)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.4 -0.250002)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.4 0.25)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "BIAS")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -1.4 0.749998)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "PGOOD")
			(pintype "unspecified+no_connect")
		)
		(pad "5" smd rect
			(at -0.749998 1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U3-RT)")
			(pinfunction "RT")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.25 1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "EN_UVLO_SYNC")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0.250002 1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.750001 1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U3-COMP)")
			(pinfunction "COMP")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 1.4 0.749998)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(U3-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 1.4 0.25)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U3-SS)")
			(pinfunction "SS")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 1.4 -0.250002)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 1.4 -0.750001)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0.750001 -1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 0.250002 -1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "12vpower")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at -0.25 -1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(U3-NC-Pad15)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd rect
			(at -0.749998 -1.4 90)
			(size 0.599999 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 1.659999 1.659999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "EP")
			(pintype "unspecified")
		)
		(pad "18" thru_hole circle
			(at 0.0254 0)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
		)
		(pad "19" thru_hole circle
			(at 0.579999 0.579999)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
		)
		(pad "20" thru_hole circle
			(at -0.579999 0.579999)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
		)
		(pad "21" thru_hole circle
			(at -0.579999 -0.579999)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
		)
		(pad "22" thru_hole circle
			(at 0.579999 -0.579999)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 88.9474 62.9265 90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k RK73B2ETTD104J"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 5 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 52.9 40 180)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D2"
			(at 0 -4.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "B540C-13-F"
			(at 0 4.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0 270)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 25 "18V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.4 0 270)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 10 "12vpower")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "F.Cu")
		(at 100.84115 64.6266)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D3"
			(at -5.7404 1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -5.7404 1.143 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 18 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 6 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 87.8332 35.9918 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0.8929 -1.7272 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf-50v-x7r 08055C104K4T2A"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2127659574)
			(net 1 "5v")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2127659574)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 52.8 31.4 180)
		(descr "JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J2"
			(at -3.9316 8.8138 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at -3.6522 12.5222 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 3.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 15 "GND2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.8)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12vpower")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.6)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 98.5 116.1 -90)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D15"
			(at 0 -4.1 -90)
			(layer "F.SilkS")
		)
		(property "Value" "ES5GC"
			(at 0 4.2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "+48V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.4 0)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 15 "GND2")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 60.536321 45.220001 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U3-SS)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 68.2896 62.9519 90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k RK73B2ETTD104J"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 8 "Net-(D7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "F.Cu")
		(at 81.27975 64.5758)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D1"
			(at -5.675 1.2446 0)
			(layer "F.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -5.6496 1.2192 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 18 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0)
			(size 3.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 5 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 46.629999 48.17)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "12vpower")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:INF-PG-TO247-3"
		(layer "F.Cu")
		(at 43.36 73.2 -90)
		(descr "Original name INF-PG-TO247-3\n\nMax Component Height - 25.57mm")
		(property "Reference" "Q4"
			(at -3 -9.25 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "IMW65R050M2H "
			(at 0.25 2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:INF-PG-TO247-3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ooo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OptiMOS 3 Power-Transistor, VDS 100V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 -5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D6-A)")
			(pinfunction "GATE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "DRAIN")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 0 5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "SOURCE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 110.85 42.144 90)
		(descr "JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J8"
			(at 6.3554 -1.8078 0)
			(layer "F.SilkS")
		)
		(property "Value" "JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 1.25 10.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 3.45 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 17 "pwm-in")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "to-sb-esp-gnd1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 114.6 32)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 104.267 49.53 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C7"
			(at 0.8382 4.3942 -90)
			(layer "F.SilkS")
		)
		(property "Value" "220uf16v RD1C227M6L011M18"
			(at 1.25 4.4 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5v")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.6)
			(thermal_bridge_angle 90)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D14.0mm_P5.00mm"
		(layer "F.Cu")
		(at 108 93)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=14mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 14mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 2.5654 -8.509 90)
			(layer "F.SilkS")
		)
		(property "Value" "CAMION Photo Flash 100µF 330V"
			(at -5.312959 4.133706 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D14.0mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.667 0.1524 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(thermal_bridge_width 1.2)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D14.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 74 54.3 180)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 -2.62 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7Ohm RC2512JK-7W4R7L"
			(at 0 2.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 18 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 28 "Net-(U1-OUTH)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:UCC27531QDBVRQ1"
		(layer "F.Cu")
		(at 67.3 53.8 -90)
		(tags "UCC27531QDBVRQ1 ")
		(property "Reference" "U1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "UCC27531QDBVRQ1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:UCC27531QDBVRQ1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "UCC27531QDBVRQ1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DBV6_TEX DBV6_TEX-M DBV6_TEX-L")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.61925 -2.6518 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.61925 -2.6518 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4953 -1.4478 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4953 -1.4478 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.36525 -0.950001 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "unconnected-(U1-EN-Pad1)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "2" smd rect
			(at -1.36525 0 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "5v-optoout")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.36525 0.950001 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "18V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at 1.36525 0.950001 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "GND2")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.36525 0 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(D1-K)")
			(pinfunction "OUTL")
			(pintype "output")
		)
		(pad "6" smd rect
			(at 1.36525 -0.950001 270)
			(size 0.9779 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U1-OUTH)")
			(pinfunction "OUTH")
			(pintype "output")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 54.079999 51.87 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.68 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.68 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U3-COMP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 31.2 88.5 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C9"
			(at -2.159 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "C100pf500v KERKO-500 100P"
			(at 2.5 2.5 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.8)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 80.74835 59.8006 180)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at -3.0968 2.921 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7Ohm RC2512JK-7W4R7L"
			(at 0 2.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 5 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 18 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 48.7426 62.3796 90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k RK73B2ETTD104J"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 7 "Net-(D6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2222222222)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 60.536321 49.320001 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.49k"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 27 "Net-(U3-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 106.0544 30.9372)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "200"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 12 "Net-(IC5-CATHODE)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 21 "to-sb-esp-gnd1")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 114.4524 46.4058 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D13"
			(at -3.302 0.6096 0)
			(layer "F.SilkS")
		)
		(property "Value" "SM0805UGC"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 15 "GND2")
			(pinfunction "K")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(pad "2" smd roundrect
			(at 1.025 0 180)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 9 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom:3006P1103"
		(layer "F.Cu")
		(at 41.1988 104.6226 -90)
		(descr "3006P-1-103-1")
		(tags "Variable Resistor")
		(property "Reference" "VR1"
			(at 9.1186 5.6896 -90)
			(layer "F.SilkS")
		)
		(property "Value" "3006P-1-103"
			(at 7.235 1.015 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "custom:3006P1103"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "15 turn cermet trimmer,10K 19mm 750mW"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "3006P-1-103"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/3006p-1-103/bourns"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "6.6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Bourns"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "3006P-1-103"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "652-3006P-1-103"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/3006P-1-103?qs=UAOLv9jeCFKRkysCp44wkQ%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 9.1186 5.6896 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.217 1.217)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(VR1-CCW)")
			(pinfunction "CCW")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 2.54 270)
			(size 1.217 1.217)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J7-Pin_2)")
			(pinfunction "WIPER")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 12.7 0 270)
			(size 1.217 1.217)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "CW")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "3006P-1-103.stp"
			(offset
				(xyz 6.499999902 -1.289999942 -0.1199999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Library:INF-PG-TO247-3"
		(layer "F.Cu")
		(at 103 73.2 -90)
		(descr "Original name INF-PG-TO247-3\n\nMax Component Height - 25.57mm")
		(property "Reference" "Q2"
			(at -3 -9.25 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "IMW65R050M2H "
			(at 0.25 2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:INF-PG-TO247-3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ooo"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OptiMOS 3 Power-Transistor, VDS 100V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 -5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-A)")
			(pinfunction "GATE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "spark-minus-to-drain")
			(pinfunction "DRAIN")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 0 5.44 270)
			(size 2.16 2.16)
			(drill 1.56)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "GND2")
			(pinfunction "SOURCE")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 100.41135 59.8006 180)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at -3.173 2.8702 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7Ohm RC2512JK-7W4R7L"
			(at 0 2.62 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 6 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 180)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1785707143)
			(net 18 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 114.6 117)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "H4"
			(at 3.302 -3.581399 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 67.1 48.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.68 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "GND2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "18V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC"
		(layer "F.Cu")
		(at 107.9 105.5)
		(descr "Diode SMC (DO-214AB)")
		(tags "Diode SMC (DO-214AB)")
		(property "Reference" "D20"
			(at 0 -4.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "ES5GC"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.9 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4 0 90)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "+48V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.4 0 90)
			(size 3.3 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 15 "GND2")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 110.85 53.0206 90)
		(descr "JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J15"
			(at -4.084 -1.884 180)
			(layer "F.SilkS")
		)
		(property "Value" "JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 1.25 10.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 3.45 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 15 "GND2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "5v")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMC_Handsoldering"
		(layer "B.Cu")
		(at 66.8782 114.9408 -90)
		(descr "Diode SMC (DO-214AB) Handsoldering")
		(tags "Diode SMC (DO-214AB) Handsoldering")
		(property "Reference" "D17"
			(at -7.62 -0.0254 0)
			(layer "B.SilkS")
		)
		(property "Value" "TVS Diode 3kw"
			(at 0 -4.2 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMC_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 3.3 4.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07575757576)
			(net 2 "+48V")
			(pinfunction "A1")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 2)
			(thermal_gap 0.3)
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 3.3 4.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07575757576)
			(net 15 "GND2")
			(pinfunction "A2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 2)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 94.8475 47.744 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at -3.0365 0.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf-50v-x7r 08055C104K4T2A"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 1 "5v")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 37.3634 117.5897 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 1.85 90)
			(layer "B.SilkS")
		)
		(property "Value" "47pf50v 08055C470KAT2A"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1778 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1886792453)
			(net 20 "Net-(J7-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1886792453)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.4)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "B.Cu")
		(at 34.5948 46.9246 -90)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D19"
			(at 6.176 -0.1016 90)
			(layer "B.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at 0.1416 -4.9114 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 6.176 -0.1016 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0 270)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1388888889)
			(net 14 "Net-(D18-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0 270)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1388888889)
			(net 15 "GND2")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 40.9 33.5 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -2.9933 0.508 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf-50v-x7r 08055C104K4T2A"
			(at -0.0469 -1.8542 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 14 "Net-(D18-K)")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.4)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "B.Cu")
		(at 32.0548 39.3954 180)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D18"
			(at -5.969 0.0508 0)
			(layer "B.SilkS")
		)
		(property "Value" "60v3ASchottky B360A-E3/61T"
			(at -55.8546 -4.4704 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA_Handsoldering"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.07413 -0.37567 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0 180)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1388888889)
			(net 14 "Net-(D18-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0 180)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1388888889)
			(net 10 "12vpower")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 51.55 28.55)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf-50v-x7r 08055C104K4T2A"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 10 "12vpower")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 88.2904 47.744 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0.1309 -1.7606 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf-50v-x7r 08055C104K4T2A"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "根目录")
		(sheetfile "evo-cube-pulseboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.0801 0.0174 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 10 "12vpower")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2127659574)
			(net 15 "GND2")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.3)
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 121.6 67.056)
		(end 121.6 117)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.6 117)
		(end 22.6 32)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.6 32)
		(mid 24.650253 27.050253)
		(end 29.6 25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 121.6 117)
		(mid 119.549747 121.949747)
		(end 114.6 124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29.6 25)
		(end 114.6 25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.6 32)
		(end 121.6 67.056)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.6 25)
		(mid 119.549747 27.050253)
		(end 121.6 32)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 29.6 124)
		(mid 24.650253 121.949747)
		(end 22.6 117)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.6 124)
		(end 29.6 124)
		(layer "Edge.Cuts")
	)
	(gr_text "-Fan+"
		(at 39.1668 39.3954 180)
		(layer "F.SilkS")
	)
	(gr_text "S   D   G"
		(at 36.07855 69.4752 0)
		(layer "F.SilkS")
	)
	(gr_text "+ 12v -"
		(at 34.036 53.086 270)
		(layer "F.SilkS")
	)
	(gr_text "PWM\n+ -"
		(at 107.6706 42.5196 90)
		(layer "F.SilkS")
	)
	(gr_text "S   D   G"
		(at 95.87015 69.5006 0)
		(layer "F.SilkS")
	)
	(gr_text "+-"
		(at 106.6292 53.4924 -90)
		(layer "F.SilkS")
	)
	(gr_text "5v Out"
		(at 112.395 57.531 0)
		(layer "F.SilkS")
	)
	(gr_text "Spark\n+     -"
		(at 73.6854 97.5868 0)
		(layer "F.SilkS")
	)
	(gr_text "DANGER!\nHigh Current\nHigh Voltage"
		(at 98.3 106.9565 90)
		(layer "F.SilkS")
	)
	(gr_text "S   D   G"
		(at 77.5 69.6 0)
		(layer "F.SilkS")
	)
	(gr_text "S   D   G"
		(at 58.2 69.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Power\n-     +"
		(at 51.4604 97.3836 0)
		(layer "F.SilkS")
	)
	(zone
		(net 15)
		(net_name "GND2")
		(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.8)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 5)
		)
		(polygon
			(pts
				(xy 127.124189 20.092286) (xy 126.955188 130.714413) (xy 17.75015 130.811987) (xy 17.80095 20.756192)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+48V")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 1.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 4)
		)
		(polygon
			(pts
				(xy 58.993788 103.076366) (xy 74.398888 103.076366) (xy 75.719688 104.397166) (xy 75.719688 116.563766)
				(xy 74.828677 117.454777) (xy 58.696534 117.550622) (xy 57.698388 116.552476) (xy 57.698388 104.371766)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+48V")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads yes
			(clearance 1.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 3)
		)
		(polygon
			(pts
				(xy 115.745153 117.045913) (xy 52.679641 117.076597) (xy 29.257922 117.087992) (xy 29.271859 111.607628)
				(xy 29.325989 90.322437) (xy 29.355704 78.637672) (xy 29.393443 63.797513) (xy 115.859918 63.617041)
			)
		)
	)
	(zone
		(net 10)
		(net_name "12vpower")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.8)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 5)
		)
		(polygon
			(pts
				(xy 100.971231 28.525828) (xy 101.028624 49.758497) (xy 89.408 49.7586) (xy 87.35391 51.790114)
				(xy 87.319969 56.8768) (xy 27.23935 56.8768) (xy 27.23935 28.657103)
			)
		)
	)
	(zone
		(net 3)
		(net_name "spark-minus-to-drain")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads yes
			(clearance 1.2)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 3)
		)
		(polygon
			(pts
				(xy 116.046031 117.983564) (xy 28.870414 118.025977) (xy 29.006175 64.641163) (xy 116.161 64.459255)
			)
		)
	)
)
