(module 2506031017Y0 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_25_0603_FRT (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.043in/1.092mm" (at 3.9243 0) (layer Cmts.User))
  (fp_text user "0.097in/2.464mm" (at 0 -3.5941) (layer Cmts.User))
  (fp_text user "0.021in/0.533mm" (at 0 3.5941) (layer Cmts.User))
  (pad 1 smd rect (at -0.7493 0) (size 0.9652 1.0922) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.7493 0) (size 0.9652 1.0922) (layers F.Cu F.Paste F.Mask))
)
