(module 250R05L101GV4T (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CAP_R05_JOD (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.013in/0.33mm" (at 3.3655 0) (layer Cmts.User))
  (fp_text user "0.053in/1.346mm" (at 0 -3.2131) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at 0 3.2131) (layer Cmts.User))
  (pad 1 smd rect (at -0.3937 0) (size 0.5588 0.3302) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.3937 0) (size 0.5588 0.3302) (layers F.Cu F.Paste F.Mask))
)
