(module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 645BD371)
  (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
  (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
  (fp_text reference REF** (at 3.75 -9.25) (layer F.SilkS))
  (pad 2 thru_hole circle (at 7.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
