(module C_2220_5650Metric (layer F.Cu) (tedit 5F68FEEE)
  (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
  (tags capacitor)
  (attr smd)
  (fp_text reference REF** (at 0 -3.65) (layer F.SilkS))
  (pad 1 smd roundrect (at -2.55 0) (size 1.8 5.4) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.138889))
  (pad 2 smd roundrect (at 2.55 0) (size 1.8 5.4) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.138889))
  (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)