(module C_Disc_D8.0mm_W5.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF0)
  (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
  (tags "C Disc series Radial pin pitch 7.50mm  diameter 8mm width 5.0mm Capacitor")
  (fp_text reference REF** (at 3.75 -3.75) (layer F.SilkS))
  (fp_text value C_Disc_D8.0mm_W5.0mm_P7.50mm (at 3.75 3.75) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (fp_text user %R (at 3.75 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D8.0mm_W5.0mm_P7.50mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)