(module C_Radial_D10.0mm_H16.0mm_P5.00mm (layer F.Cu) (tedit 5BC5C9BA)
  (descr "C, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=16mm, Non-Polar Electrolytic Capacitor")
  (tags "C Radial series Radial pin pitch 5.00mm diameter 10mm height 16mm Non-Polar Electrolytic Capacitor")
  (fp_text reference REF** (at 2.5 -6.25) (layer F.SilkS))
  (fp_text value C_Radial_D10.0mm_H16.0mm_P5.00mm (at 2.5 6.25) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.5 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Radial_D10.0mm_H16.0mm_P5.00mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)