(module Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT (layer F.Cu) (tedit 59FE19B9)
  (descr "DCDC-Converter, TRACO, TMR 1-xxxx, Single output, Rev. March 21.2016")
  (tags "DCDC-Converter TRACO TMR1-xxxx Single_output")
  (fp_text reference REF** (at -0.63 -3.83) (layer F.SilkS))
  (fp_text value Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT (at 6.5 6.5) (layer F.Fab))
  (fp_text user %R (at 5.91 3) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.5 3) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0) (size 1.5 3) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 7.62 0) (size 1.5 3) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 12.7 0) (size 1.5 3) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TMR-1-xxxx_Single_THT.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
