(footprint "DQN0004A-MFG" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "TPS7A0318PDQNR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value DQN0004A-MFG (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "Designator9" (at -1.2954 -2.0066 unlocked) (layer "F.SilkS"))
  (pad "1" smd circle (at -0.505 -0.329999) (size 0.279001 0.279001) (layers "F.Cu"))
  (pad "2" smd circle (at -0.505 0.329999) (size 0.279001 0.279001) (layers "F.Cu"))
  (pad "3" smd circle (at 0.459265 0.345547) (size 0.251013 0.251013) (layers "F.Cu"))
  (pad "4" smd circle (at 0.459265 -0.345547) (size 0.251013 0.251013) (layers "F.Cu"))
  (pad "5" smd rect (at 0 0 315) (size 0.579999 0.579999) (layers "F.Cu"))
)
