(module G3VM-201G1 (layer F.Cu)
  (fp_text reference REF** (at 3.075 1.27) (layer F.SilkS))
  (fp_text value G-SOP4_OMR (at 3.075 1.27) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer Cmts.User))
  (fp_text user "0.031in/0.8mm" (at 9.198001 0) (layer Cmts.User))
  (fp_text user "0.242in/6.15mm" (at 3.075 -3.093) (layer Cmts.User))
  (fp_text user "0.047in/1.2mm" (at 0 5.633) (layer Cmts.User))
  (fp_text user "*" (at 1.129001 0) (layer F.Fab))
  (fp_text user "*" (at 0 -1.162) (layer F.SilkS))
  (pad 1 smd rect (at 0 0) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 2.54) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 6.15 2.54) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 6.15 0) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask))
)
