(module GMC04X7R101K6R3NT (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CAP_GMC04_CCE (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.022in/0.559mm" (at 3.5687 0) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 0 -3.3274) (layer Cmts.User))
  (fp_text user "0.013in/0.33mm" (at 0 3.3274) (layer Cmts.User))
  (pad 1 smd rect (at -0.5207 0) (size 0.7112 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.5207 0) (size 0.7112 0.5588) (layers F.Cu F.Paste F.Mask))
)
