(module NSS12201LT1G (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOT-23-3_1P4X3P040_ONS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.022in/0.559mm" (at 0 -3.0988) (layer Cmts.User))
  (fp_text user "0.052in/1.321mm" (at 3.302 1.016) (layer Cmts.User))
  (pad 1 smd rect (at -0.9525 1.016) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.9525 1.016) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -1.016) (size 0.5588 1.3208) (layers F.Cu F.Paste F.Mask))
)
