(module Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148)
  (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
  (tags "relay Sanyu SRD form C")
  (fp_text reference REF** (at 8.1 9.2) (layer F.SilkS))
  (fp_text value Relay_SPDT_SANYOU_SRD_Series_Form_C (at 8 -9.6) (layer F.Fab))
  (fp_text user 1 (at 0 -2.3) (layer F.Fab))
  (fp_text user %R (at 7.1 0.025) (layer F.Fab))
  (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
