(module Rotary_Encoder:RotaryEncoder_Alps_EC12E_Vertical_H20mm (layer F.Cu) (tedit 62BDA348)
  (descr "Alps rotary encoder, EC12E..., vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC12E/EC12E1240405.html")
  (tags "rotary encoder")
  (fp_text reference REF** (at 2.8 -4.7) (layer F.SilkS))
  (fp_text value RotaryEncoder_Alps_EC12E_Vertical_H20mm (at 7.5 10.4) (layer F.Fab))
  (pad A thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad C thru_hole circle (at 0 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad B thru_hole circle (at 0 5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad MP1 thru_hole rect (at 7.5 -3.1) (size 3 2.5) (drill oval 2.5 2) (layers *.Cu *.Mask))
  (pad MP2 thru_hole rect (at 7.5 8.1) (size 3 2.5) (drill oval 2.5 2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC12E_Vertical_H20mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
