(module R_0815_2038Metric (layer F.Cu) (tedit 62BDE7AC)
  (descr "Resistor SMD 0815 (2038 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.susumu.co.jp/common/pdf/n_catalog_partition07_en.pdf), generated with kicad-footprint-generator")
  (tags resistor)
  (attr smd)
  (fp_text reference REF** (at 0 -2.98) (layer F.SilkS))
  (fp_text value R_0815_2038Metric (at 0 2.98) (layer F.Fab))
  (pad 1 smd roundrect (at -0.9375 0) (size 1.025 4.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902))
  (pad 2 smd roundrect (at 0.9375 0) (size 1.025 4.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902))
  (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0815_2038Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
