(module L_1008_2520Metric (layer F.Cu) (tedit 62D6981A)
  (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
  (tags inductor)
  (attr smd)
  (fp_text reference REF** (at 0 -2.05) (layer F.SilkS))
  (fp_text value L_1008_2520Metric (at 0 2.05) (layer F.Fab))
  (pad 1 smd roundrect (at -1.075 0) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 2 smd roundrect (at 1.075 0) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
