(footprint "SOT323_BSS816NWH6327XTSA1_INF" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "BSS816NWH6327XTSA1 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value SOT323_BSS816NWH6327XTSA1_INF (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -0.649999 1.0492) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0.649999 1.0492) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 0 -1.0492) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask"))
)
