(module Button_Switch_THT:SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 633AF728)
  (descr "1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
  (tags "DIP Switch SPST Slide 7.62mm 300mil")
  (fp_text reference REF** (at 3.81 -3.42) (layer F.SilkS))
  (fp_text value SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm (at 3.81 3.42) (layer F.Fab))
  (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
  (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
