(module Button_Switch_SMD:SW_Push_SPST_NO_Alps_SKRK (layer F.Cu) (tedit 5C2A8900)
  (descr http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKRK/SKRKAHE020.html)
  (tags "SMD SMT button")
  (attr smd)
  (fp_text reference REF** (at 0 -2.25) (layer F.SilkS))
  (fp_text value SW_Push_SPST_NO_Alps_SKRK (at 0 2.5) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 1 smd roundrect (at -2.1 0) (size 0.8 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 2.1 0) (size 0.8 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_Push_SPST_NO_Alps_SKRK.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
