(footprint "TC2030-IDC" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.445 -0.635 180) (layer "F.SilkS"))
  (fp_text value "TC2030-IDC" (at -5.08 -3.81 180) (layer "F.Fab"))
  (pad "" np_thru_hole circle (at -2.54 -2.54) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at -2.54 0) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at -2.54 2.54) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 0.635 -2.54) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 0.635 2.54) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 2.54 -1.016) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 2.54 1.016) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
  (pad "1" smd circle (at -1.27 0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd circle (at -1.27 -0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd circle (at 0 0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd circle (at 0 -0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd circle (at 1.27 0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd circle (at 1.27 -0.635) (size 0.7874 0.7874) (layers "F.Cu" "F.Paste" "F.Mask"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.27 -0.635)
        (xy 1.27 -0.635)
        (xy 1.27 0.635)
        (xy -1.27 0.635)
      )
    )
  )
  (model "C:/Users/davidh/Documents/----Downloaded Electronics Libraries/Debugger/Tag-Connect/TC2030-IDC.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
