(module Package_TO_SOT_SMD:TO-252-2 (layer F.Cu) (tedit 5A70A390)
  (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
  (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
  (attr smd)
  (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
  (fp_text value TO-252-2 (at 0 4.5) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
  (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
  (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
  (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
  (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
