(footprint "Texas_DQK"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Texas WSON-6 DQK, http://www.ti.com/lit/ds/symlink/csd16301q2.pdf")
	(tags "Texas WSON6 2x2mm")
	(property "Reference" "REF**"
		(at 0 -1.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DQK"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0 -0.325)
		(size 0.9 0.86)
		(layers "F.Paste")
		(roundrect_rratio 0.058)
	)
	(pad "" smd roundrect
		(at 0.095 0.65)
		(size 0.7 0.29)
		(layers "F.Paste")
		(roundrect_rratio 0.172)
	)
	(pad "1" smd roundrect
		(at -0.975 -0.65)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "2" smd roundrect
		(at -0.975 0)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "3" smd roundrect
		(at -0.975 0.65)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "4" smd roundrect
		(at 0.975 0.65)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "5" smd roundrect
		(at 0.975 0)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "6" smd roundrect
		(at 0.975 -0.65)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "7" smd roundrect
		(at 0.095 0.65)
		(size 0.75 0.3)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.167)
	)
	(pad "8" smd roundrect
		(at 0 -0.325)
		(size 1 0.95)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.053)
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DQK.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)